**PARA LOS ROUTERS DENTRO DE ÁREA**

interface/bridge/add name=loopback

ip address/add interface=loopback address=10.255.255.14

routing/id/add name=id\_ospf select-dynamic-id=only-loopback

routing/ospf/instance/add name=ospf router-id=id\_ospf

routing/ospf/area/add name=areaC area-id=0.0.0.3 type=stub instance=ospf

**PARA LOS ROUTERS BORDES DE ÁREA → Router ABR (no summaries)**

interface/bridge/add name=loopback

ip address/add interface=loopback address=10.255.255.3

routing/id/add name=id\_ospf select-dynamic-id=only-loopback

routing/ospf/instance/add name=ospf router-id=id\_ospf

routing/ospf/area/add name=areaC instance=ospf area-id=0.0.0.3 type=stub no-summaries default-cost=1

routing/ospf/area/range/add area=areaA prefix=10.3.15.0/24

routing/ospf/interface-template/add area=backbone interfaces=ether6 type=ptp

routing/ospf/interface-template/add area=areaA interfaces=ether3 type=ptp

**PARA LOS ROUTERS SIN AREA (BACKBONE)**

interface/bridge/add name=loopback

ip address/add interface=loopback address=10.255.255.4

routing/id/add name=id\_ospf select-dynamic-id=only-loopback

routing/ospf/instance/add name=ospf router-id=id\_ospf

routing/ospf/area/add name=backbone

routing/ospf/interface-template/add area=backbone interfaces=ether1 type=ptp



