**R1:**

interface/bridge/add name=bridge1 vlan-filtering=yes

interface/bridge/port add bridge=bridge1 interface=ether6

interface/bridge/port add bridge=bridge1 interface=ether1 pvid=10

interface/bridge/port add bridge=bridge1 interface=ether2 pvid=20

interface/bridge/port add bridge=bridge1 interface=ether3 pvid=30

interface/bridge/vlan/add tagged=ether6,bridge1 vlan-ids=10 untagged=ether1 bridge=bridge1

interface/bridge/vlan/add tagged=ether6,bridge1 vlan-ids=20 untagged=ether2 bridge=bridge1

interface/bridge/vlan/add tagged=ether6,bridge1 vlan-ids=40 bridge=bridge1

interface/vlan/add interface=bridge1 vlan-id=10 name=vlan10

interface/vlan/add interface=bridge1 vlan-id=20 name=vlan20

interface/vlan/add interface=bridge1 vlan-id=30 name=vlan30

…..

ipv6/address/add eui-64=yes advertise=yes interface=vlan10 address=2001:db8:a::/64

ipv6/address/add eui-64=yes advertise=yes interface=vlan20 address=2001:db8:b::/64

ipv6/address/add eui-64=yes advertise=yes interface=vlan30 address=2001:db8:c::/64

….

ip/address/add interface=vlan10 address=192.168.1.1/24

ip/address/add interface=vlan20 address=192.168.2.1/24

ip/address/add interface=vlan30 address=192.168.3.1/24

…..

ipv6/nd/set 0 ra-interval=10-30

ip/dhcp-server/setup

* vlan10
* vlan20
* …..

**R2:**

interface/bridge/add name=bridge1 vlan-filtering=yes

interface/bridge/port add bridge=bridge1 interface=ether6

interface/bridge/port add bridge=bridge1 interface=ether5

interface/bridge/port add bridge=bridge1 interface=ether4

interface/bridge/vlan/add bridge=bridge1 tagged=ether4,ether5,ether6 vlan-ids=10

interface/bridge/vlan/add bridge=bridge1 tagged=ether4,ether5,ether6 vlan-ids=20

interface/bridge/vlan/add bridge=bridge1 tagged=ether4,ether5,ether6 vlan-ids=30

….

**R3:**

interface/bridge/add name=bridge1 vlan-filtering=yes

interface/bridge/port add bridge=bridge1 interface=ether6

interface/bridge/port add bridge=bridge1 interface=ether1 pvid=20

interface/bridge/port add bridge=bridge1 interface=ether2 pvid=10

interface/bridge/port add bridge=bridge1 interface=ether3 pvid=30

interface/bridge/vlan/add bridge=bridge1 tagged=ether6 untagged=ether1 vlan-ids=20

interface/bridge/vlan/add bridge=bridge1 tagged=ether6 untagged=ether2 vlan-ids=10

interface/bridge/vlan/add bridge=bridge1 tagged=ether6 untagged=ether3 vlan-ids=30

**R5:**

interface/bridge/add name=bridge1 vlan-filtering=yes

interface/bridge/port add bridge=bridge1 interface=ether6

interface/bridge/port add bridge=bridge1 interface=ether1 pvid=50

interface/bridge/port add bridge=bridge1 interface=ether2 pvid=40

interface/bridge/port add bridge=bridge1 interface=ether3 pvid=60

interface/bridge/vlan/add bridge=bridge1 tagged=ether6 untagged=ether1 vlan-ids=50

interface/bridge/vlan/add bridge=bridge1 tagged=ether6 untagged=ether2 vlan-ids=40

interface/bridge/vlan/add bridge=bridge1 tagged=ether6 untagged=ether3 vlan-ids=60

