**R1:**

interface/bridge/add name=bridge1 vlan-filtering=yes

interface/bridge/port add bridge=bridge1 interface=ether6

interface/bridge/port add bridge=bridge1 interface=ether5

interface/bridge/port add bridge=bridge1 interface=ether4

interface/bridge/port add bridge=bridge1 interface=ether1 pvid=12

interface/bridge/port add bridge=bridge1 interface=ether2 pvid=13

interface/bridge/vlan/add tagged=ether4,ether6,ether5,bridge1 vlan-ids=12 untagged=ether1 bridge=bridge1

interface/bridge/vlan/add tagged=ether4,ether6,ether5,bridge1 vlan-ids=13 untagged=ether2 bridge=bridge1

interface/bridge/vlan/add tagged=ether4,ether6,ether5,bridge1 vlan-ids=10 bridge=bridge1

interface/bridge/vlan/add tagged=ether4,ether6,ether5,bridge1 vlan-ids=11 bridge=bridge1

interface/bridge/vlan/add tagged=ether4,ether6,ether5,bridge1 vlan-ids=14 bridge=bridge1

interface/bridge/vlan/add tagged=ether4,ether6,ether5,bridge1 vlan-ids=15 bridge=bridge1

interface/vlan/add interface=bridge1 vlan-id=10 name=vlan10

interface/vlan/add interface=bridge1 vlan-id=11 name=vlan11

interface/vlan/add interface=bridge1 vlan-id=12 name=vlan12

interface/vlan/add interface=bridge1 vlan-id=13 name=vlan13

interface/vlan/add interface=bridge1 vlan-id=14 name=vlan14

interface/vlan/add interface=bridge1 vlan-id=15 name=vlan15

ipv6/address/add eui-64=yes advertise=yes interface=vlan10 address=2001:aaaa:15::/64

ipv6/address/add eui-64=yes advertise=yes interface=vlan11 address=2001:bbbb:15::/64

ipv6/address/add eui-64=yes advertise=yes interface=vlan12 address=2001:cccc:15::/64

ipv6/address/add eui-64=yes advertise=yes interface=vlan13 address=2001:dddd:15::/64

ipv6/address/add eui-64=yes advertise=yes interface=vlan14 address=2001:eeee:15::/64

ipv6/address/add eui-64=yes advertise=yes interface=vlan15 address=2001:ffff:15::/64

ip/address/add interface=vlan10 address=10.15.10.1/24

ip/address/add interface=vlan11 address=10.15.11.1/24

ip/address/add interface=vlan12 address=10.15.12.1/24

ip/address/add interface=vlan13 address=10.15.13.1/24

ip/address/add interface=vlan14 address=10.15.14.1/24

ip/address/add interface=vlan15 address=10.15.15.1/24

ipv6/nd/set 0 ra-interval=10-15

ip/dhcp-server/setup

**R2:**

interface/bridge/add name=bridge1 vlan-filtering=yes

interface/bridge/port add bridge=bridge1 interface=ether6

interface/bridge/port add bridge=bridge1 interface=ether5

interface/bridge/port add bridge=bridge1 interface=ether4

interface/bridge/vlan/add bridge=bridge1 tagged=ether4,ether5,ether6 vlan-ids=10

interface/bridge/vlan/add bridge=bridge1 tagged=ether4,ether5,ether6 vlan-ids=20

interface/bridge/vlan/add bridge=bridge1 tagged=ether4,ether5,ether6 vlan-ids=30

….

**R3:**

interface/bridge/add name=bridge1 vlan-filtering=yes

interface/bridge/port add bridge=bridge1 interface=ether5

interface/bridge/port add bridge=bridge1 interface=ether6

interface/bridge/port add bridge=bridge1 interface=ether1 pvid=10

interface/bridge/port add bridge=bridge1 interface=ether2 pvid=11

interface/bridge/vlan/add bridge=bridge1 tagged=ether5 untagged=ether1 vlan-ids=10

interface/bridge/vlan/add bridge=bridge1 tagged=ether5 untagged=ether2 vlan-ids=11

**R5:**

interface/bridge/add name=bridge1 vlan-filtering=yes

interface/bridge/port add bridge=bridge1 interface=ether6

interface/bridge/port add bridge=bridge1 interface=ether1 pvid=50

interface/bridge/port add bridge=bridge1 interface=ether2 pvid=40

interface/bridge/port add bridge=bridge1 interface=ether3 pvid=60

interface/bridge/vlan/add bridge=bridge1 tagged=ether6 untagged=ether1 vlan-ids=50

interface/bridge/vlan/add bridge=bridge1 tagged=ether6 untagged=ether2 vlan-ids=40

interface/bridge/vlan/add bridge=bridge1 tagged=ether6 untagged=ether3 vlan-ids=60

